(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "+5V")
  (net 3 "R1_R2")
  (net 4 "R2_R3")
  (net 5 "LED_IN")
  (net 6 "LED_OUT")
  (net 7 "Net-(D1-Pad2)")
  (net 8 "Net-(D3-Pad2)")
  (net 9 "Net-(D4-Pad2)")
  (net 10 "Net-(D5-Pad2)")
  (net 11 "Net-(D7-Pad2)")
  (footprint "RGBW_LED_circular_panel_for_Stealthburner:WS2812B-2020" (layer "F.Cu")
    (tedit 61CF2C92)
    (at 149.69 95.57)
    (property "Sheetfile" "RGBW_LED_circular_panel_for_Stealthburner.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 0 2) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 0 -2) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at 0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D1-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at -0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "LED_IN") (pinfunction "DIN") (pintype "input"))
    (model "${KIPRJMOD}/LED_WS2812_2020.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "RGBW_LED_circular_panel_for_Stealthburner:WS2812B-2020" (layer "F.Cu")
    (tedit 61CF2C92)
    (at 148.23 98.09)
    (property "Sheetfile" "RGBW_LED_circular_panel_for_Stealthburner.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at 0 2) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 0 -2) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at 0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "R1_R2") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at -0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D1-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KIPRJMOD}/LED_WS2812_2020.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "RGBW_LED_circular_panel_for_Stealthburner:WS2812B-2020" (layer "F.Cu")
    (tedit 61CF2C92)
    (at 152.85 98.09)
    (property "Sheetfile" "RGBW_LED_circular_panel_for_Stealthburner.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D4" (at 0 2) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 0 -2) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at 0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D4-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at -0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D3-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KIPRJMOD}/LED_WS2812_2020.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "RGBW_LED_circular_panel_for_Stealthburner:WS2812B-2020" (layer "F.Cu")
    (tedit 61CF2C92)
    (at 151.4 100.6)
    (property "Sheetfile" "RGBW_LED_circular_panel_for_Stealthburner.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D5" (at 0 2) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 0 -2) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at 0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D5-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at -0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D4-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KIPRJMOD}/LED_WS2812_2020.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "RGBW_LED_circular_panel_for_Stealthburner:WS2812B-2020" (layer "F.Cu")
    (tedit 61CF2C92)
    (at 149.95 103.11)
    (property "Sheetfile" "RGBW_LED_circular_panel_for_Stealthburner.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D6" (at 0 2) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 0 -2) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at 0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "R2_R3") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at -0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D5-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KIPRJMOD}/LED_WS2812_2020.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "RGBW_LED_circular_panel_for_Stealthburner:WS2812B-2020" (layer "F.Cu")
    (tedit 61CF2C92)
    (at 156.02 100.6)
    (property "Sheetfile" "RGBW_LED_circular_panel_for_Stealthburner.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D7" (at 0 2) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 0 -2) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at 0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D7-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at -0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "R2_R3") (pinfunction "DIN") (pintype "input"))
    (model "${KIPRJMOD}/LED_WS2812_2020.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "RGBW_LED_circular_panel_for_Stealthburner:WS2812B-2020" (layer "F.Cu")
    (tedit 61CF2C92)
    (at 154.57 103.11)
    (property "Sheetfile" "RGBW_LED_circular_panel_for_Stealthburner.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D8" (at 0 2) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 0 -2) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at 0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "LED_OUT") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at -0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D7-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KIPRJMOD}/LED_WS2812_2020.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "RGBW_LED_circular_panel_for_Stealthburner:WS2812B-2020" (layer "F.Cu")
    (tedit 61CF2C92)
    (at 154.3 95.58)
    (property "Sheetfile" "RGBW_LED_circular_panel_for_Stealthburner.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at 0 2) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 0 -2) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at 0.915 0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D3-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at -0.915 -0.55) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "R1_R2") (pinfunction "DIN") (pintype "input"))
    (model "${KIPRJMOD}/LED_WS2812_2020.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Pin_Headers:Pin_Header_Straight_2x03_Pitch2.00mm_SMD" (layer "B.Cu")
    (tedit 61C88B2D)
    (at 151.39 99.37 180)
    (descr "surface-mounted straight pin header, 2x03, 2.00mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.00mm double row")
    (property "Sheetfile" "RGBW_LED_circular_panel_for_Stealthburner.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 0 4.06 180) (layer "B.SilkS") hide)
    (fp_text value "Conn_02x03_Odd_Even" (at 0 -4.06 180) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab") hide)
    (pad "1" smd rect locked (at -2.085 2 180) (size 2.58 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect locked (at 2.085 2 180) (size 2.58 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect locked (at -2.085 0 180) (size 2.58 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "LED_IN") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect locked (at 2.085 0 180) (size 2.58 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "LED_OUT") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect locked (at -2.085 -2 180) (size 2.58 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect locked (at 2.085 -2 180) (size 2.58 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.00mm_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 148.77637 105.144263) (end 155.473632 105.144263) (layer "Edge.Cuts") (width 0.01))
  (gr_line (start 156.522948 95.361732) (end 155.473632 93.544264) (layer "Edge.Cuts") (width 0.01))
  (gr_arc (start 157.772948 97.526796) (mid 156.065416 97.069264) (end 156.522948 95.361732) (layer "Edge.Cuts") (width 0.01))
  (gr_line (start 148.77637 93.544264) (end 145.427738 99.344264) (layer "Edge.Cuts") (width 0.01))
  (gr_line (start 155.473632 105.144263) (end 158.822264 99.344264) (layer "Edge.Cuts") (width 0.01))
  (gr_line (start 145.427738 99.344264) (end 148.77637 105.144263) (layer "Edge.Cuts") (width 0.01))
  (gr_line (start 157.772948 97.526795) (end 158.822264 99.344264) (layer "Edge.Cuts") (width 0.01))
  (gr_line (start 148.77637 93.544264) (end 155.473632 93.544264) (layer "Edge.Cuts") (width 0.01))
  (gr_text "DOUT" (at 147.16 99.45 270) (layer "B.SilkS"))
  (gr_text "5V" (at 151.35 96.16) (layer "B.SilkS"))
  (gr_text "GND" (at 151.49 102.77) (layer "B.SilkS"))
  (gr_text "DIN" (at 155.53 99.38 270) (layer "B.SilkS"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.127) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 158.85 106)
        (xy 145.35 106)
        (xy 145.35 93)
        (xy 158.85 93)
      )
    )
  )
  (zone (net 2) (net_name "+5V") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.85 106)
        (xy 145.35 106)
        (xy 145.35 93)
        (xy 158.85 93)
      )
    )
  )
)
